**Digital Hanging Scale**

**Model: OCS-AF Specifications:**

|  |  |  |  |
| --- | --- | --- | --- |
| **Model** | **Cap.****(kg)** | **Resolution****(kg)** | **N.W.****(kg)** |
| **OCS-AF-003** | 30 | 0.01 | 0.95 |
| **OCS-AF-005** | 50 | 0.02 | 0.95 |
| **OCS-AF-01** | 100 | 0.05 | 0.95 |
| **OCS-AF-015** | 150 | 0.05 | 0.95 |
| **OCS-AF-02** | 200 | 0.1 | 0.95 |
| **OCS-AF-03** | 300 | 0.1 | 0.95 |

****

**Features：**

◆ **Rotating hook:** 360**°**safe rotated hook, convenient to use

◆**Enclosure:**

 NEMA 12/IP54 powder coated Die-Casting Plastic, very light, easy to bring.

◆**Multi-weighing units**:

 Kg, lb, N are selectable, kg are default unit.

* **Multi-function operation:**

Tare, Zero, Auto zero tracking, Total, Hold, Overload warning and record, Battery Operated with low battery indication, Automatic turn off , power-saving function, parameter setting and calibration through infrared remote controller.

* **Gravity regulation:**

The acceleration of gravity can be regulated through remote controller according to different places value.

* **Multi options:**

RS-232-continuous or on demand data output, user-selectable.

**Main technical data：**

|  |  |
| --- | --- |
| Accuracy Standard | According to OIML class III |
| Display | 20mm (0.8″) 5digits LCD/LED |
| Filtering | Low, Medium or High selectable |
| Units | Kilograms or Pounds or Newtons selectable |
| Resulation | 2000 to 3000 divisions standard(up to 15,000 available) |
| Zero Range | 4% F.S. |
| Tare Range | 100% F.S. |
| Overload Indication | 100% F.S. + 9e |
| Max. Safety Load | 125% F.S. |
| Ultimate Load | 400% F.S. |
| Battery Type | Fully sealed Lead-Acid battery, 4V/2Ah，AA size battery are selectable |
| Battery Life | ≥80 hours |
| Adapter | DC 4V/500mA |
| Operating Temperature Range | - 20℃ ~ + 50℃ |
| Operating Humidity  | ≤85% RH under 20℃ |
| Remote Controller Distance | Max. 15m |
| Battery of Remote Controller | 7# battery, 1.5Vⅹ2 |
| Acceleration of Gravity | Can be regulated, the default value is 9.793 |