
**Wireless weighing Indicator(USB KIT)**

**Model: 18**



**Transmitter Receiver**

**![)WL756KC(`](I]}C@FFVNZN](data:image/jpeg;base64,)** 

**Features:**

* **Palm-size:** **28x70x90**mm shell with LCD display, wireless double-sided communication(can tare,zero,calibration and parameter setting). 5 digits LCD display with backlight，digit height：12mm. Many function on LCD display( battery power,TARE,ZERO,PEAK,Stable) .
* **USB port:**  Communicate with PC,Solve many laptops without serial port problem.with the Anyweight company’s PC host computer software,not only display weigh value and stable information on the PC , also can input company’s name,complete storage ,print query and other function.
* **Power supply:** USB power supply, lithium battery optional .
* **Operatiing temperature:** -20℃ to 60℃
* **Antenna:** Intergral antenna
* **Update rate from loadcell:** 12 times per second.
* **Radio Frequency:** Standard 2.4GHz wireless module, up to 70m wireless distance，up to 128 channels available.（433MHz, 868MHz wireless module optional）.
* **Extensive use occassions:** Not only can be used with Anyweight crane scale and dynamometer, but also can communicate with any other weighing indicator with RS232 output.